Initial setup

Navigate to System → Settings → Administration and change the TCP port field to something other than 80 or 443. Then, also check the HTTP Redirect field to disable web GUI redirect rule.

DHCP

Services: DHCPv4: [LAN] → scroll to end of page → DHCP Static Mappings for this interface.